Schmidt Ocean Institute

R/V *Falkor (too)* Survey Plan Template Information

*Email to* [*mt@falkortoo.org*](mailto:mt@falkortoo.org) *&* [*leadtech@falkortoo.org*](mailto:leadtech@falkortoo.org)

*The following document is intended to guide science parties into giving key information needed during a multibeam survey so the survey goals can be best met by the ship’s crew. The information below is not required, but is intended to serve as a guide. Everything in italic should be removed and replaced with information provided by the science party.*

**Survey Info**

Date of Survey:

Estimated Start Time of Survey:

Requested Sonar:*See System Descriptions below for specifications.*

Requested Survey Speed:

* *FKt normal survey speed: 6 knots*
* *FKt high resolution survey speed: 4 knots*
* *FKt max distance coverage survey speed: 8 knots*

**Description of Survey**

*This is an opportunity to explain the goals and objectives of the survey, which may include/ answer the following prompts:*

* *Description of the feature/survey area*
* *Are the goals of the survey to explore an unknown region, to achieve the highest resolution possible, to achieve the highest coverage possible, or a combination?*
* *Has the survey area been previously surveyed? Is our goal to expand coverage or increase resolution? Mapping sonar/ resolution is helpful if known.*
* *Depth Ranges of the area if known to aid in choosing the sonar.*
* *What features, if any, should be prioritized, ex. keeping a ridge line centered.*
* *Are there any hazards to navigation that would alter how the survey is conducted, for example, rocks, uncharted areas, etc.*

**Survey Procedures**

*If you have preferences for how the survey will be carried out, you can explain them here:*

* *What support (if any) will we receive from the science party during the survey?*
* *By default, we log the ‘start/ end of survey’ as well as major settings changes. If you have any specific requirements (ie. line start/stop) please specify.*
* *How would you prefer the ship to handle turns in the survey?*
* *By default, we try to start new lines during turns so the turn data is easier to edit out during post processing, please specify if you want line changes handled a certain way.*
* *If the line coverage is different from planned, for this survey do you want us to ‘edge map’ to eliminate holes or stick to the line plan specified.*
* *If the ETA to the end of the survey is different than planned, would you like the ship to finish the survey or maintain the planned schedule?* 
  + *If the survey ended early, should we continue mapping until the scheduled time?*
  + *If the survey won't be finished by the scheduled time, should we stay longer to finish the survey or break off at the expected time?*

**Waypoints**

* *Waypoint Number, Latitude, Longitude* 
  + *D.DDD is preferred*
  + *If possible, providing the waypoints in a separate txt or csv document will speed up the process of distributing to the bridge/multibeam systems.*
* *An example is below:*

| *Waypoint #* | *Latitude (d.dddd)* | *Longitude (d.dddd)* |
| --- | --- | --- |
| *1* | *10.1234* | *-89.9876* |
| *2* | *10.5678* | *-89.5432* |
| *3* | *10.9012* | *-89.1098* |
| *4* | *10.345* | *-89.7654* |

**Map**

* *If previous multibeam data or satellite data is available a map with our projected survey lines is helpful.*

**Speed and distance**

1 Kilometer = 0.539 Nautical Miles

Rounded time

| **Speed in knots** | **1 Km**  **Time in mins** |
| --- | --- |
| .5 | 66 |
| 1 | 33 |
| 2 | 17 |
| 3 | 11 |
| 4 | 8 |
| 5 | 6.5 |
| 6 | 5.5 |

**Additional Tools:**

**System Descriptions**

**EM2040**

**Beam Width:** 0.4° Tx with 0.75° Rx

**Depth Range:** < 1m - 635m

**Falkor (too) Operating Range:** 50m - 200m

**Operating Frequency:** 200 - 700 kHz

**Swath Width:** Up to 170°

**Receiver Beams:** 1024 beams

* Our EM2040 is our shallow water multibeam that is generally used in less than 100m of water. For surveys this shallow, we will be syncing the EM2040 with our SU90 (forward facing sonar) with Konsberg’s KSYNC to ensure safe navigation of the vessel.
* For shallow water mapping (less than 100m), we require a line plan that will ensure we stay within the swath of our mapping data and must be organized clearly with the bridge prior to the survey. Near coastal mapping in shallow water must be done during the day and with clearance from the Captain.

EM2040 Estimated Depth x Swath Width

Assuming fully open beam angles and flat terrain in a 200kHz setting.

| **Depth** | **Swath Width (m)** | **Total Coverage (m)** |
| --- | --- | --- |
| 50 | 100 | 200 |
| 100 | 280 | 560 |
| 150 | 280 | 560 |
| 200 | 200 | 400 |
| 250 | 180 | 360 |
| 300 | 160 | 320 |
| 350 | 120 | 240 |
| 400 | 80 | 160 |
| 450 | 80 | 160 |
| 500 | 50 | 100 |

**EM712**

**Beam Width:** 0.25० Tx by 0.5० Rx, full performance

**Depth Range:** 3m - 3,600m

**Falkor (too) Operating Range:** 100m - 1,500m

**Operating Frequency:** 40 - 100 kHz

**Swath Width:** up to 5.5 times the depth

**Receiver Beams:** 1600 beams

* Our EM712 is our shallow- mid water multibeam that does best in 100m- 1500m of water.
* The ADCP often causes interference with the EM712, so those should be secured during EM712 surveys.
* The SU90 causes interference with the EM712, so that should be secured during EM712 surveys. In some cases, if the Bridge requires the SU90, we may need to use the EM124 for that survey.
* Performance of the 712 is affected by water depth, vessel noise, sonar cross talk, and sea state. In general, it has to be monitored more closely than our other sonars.
* For features ranging in depth from 300-2000m, we recommend running the EM712 and EM124 synchronized. This also gives the bridge the opportunity to run the SU90 sync’d with EM124.
* For line planning purposes, you can estimate a line spacing of 3x the water depth for the EM712.

EM712 Estimated Depth x Swath Width

Assuming fully open beam angles and flat terrain.

| **Depth** | **Swath Width (m)** | **Total Coverage (m)** |
| --- | --- | --- |
| 250 | 600 | 1200 |
| 500 | 1000 | 2000 |
| 750 | 1300 | 2600 |
| 1000 | 1400 | 2800 |
| 1250 | 1500 | 3000 |
| 1500 | 1500 | 3000 |
| 1750 | 1600 | 3200 |
| 2000 | 1400 | 2800 |
| 2250 | 1000 | 2000 |
| 2500 | 1000 | 2000 |
| 2750 | 1200 | 2400 |
| 3000 | 1200 | 2400 |

**EM124**

**Beam Width:** 0.5० Tx by 1० Rx

**Depth Range:** 20m - 11,000m

**Falkor (too) Operating Range:** 1,500m - 11,000m

**Nominal Frequency:** 12 kHz

**Operating Frequency:** 10.5 - 13.5 kHz

**Swath Width:** up to 6 times the depth

**Receiver Beams:** 1600 beams

* Our EM124 is our mid- deep water multibeam that can be synchronized to work with our Sub Bottom Sonar between pings to simultaneously log multibeam and sub bottom data.
* The EM124 does not receive interference from the ADCPs or SU90, which allows those to also be running simultaneously without losing ping density from synchronizing multiple echosounders.
* For line planning purposes, in general you can estimate line spacing of 4x the water depth for the EM124.

EM124 Estimated Depth x Swath Width

Assuming fully open beam angles and flat terrain.

| **Depth** | **Swath Width (m)** | **Total Coverage (m)** |
| --- | --- | --- |
| 250 | 1000 | 2000 |
| 500 | 1250 | 2500 |
| 1000 | 2500 | 5000 |
| 1500 | 4000 | 8000 |
| 2000 | 5000 | 10000 |
| 2500 | 6250 | 12500 |
| 3000 | 7000 | 14000 |
| 3500 | 8000 | 16000 |
| 4000 | 9000 | 18000 |
| 4500 | 9500 | 19000 |
| 5000 | 10000 | 20000 |
| 6000 | 11000 | 22000 |
| 7000 | 12000 | 24000 |
| 8000 | 9000 | 18000 |